Project Name:

testservice

Client Name:

tc

Capacity:

tc

### 1. Manual Screen

|  |  |
| --- | --- |
|  |  |
| Manufacturer | Factory |
| Quantity | 1 |
| Operation | Manual |

|  |  |
| --- | --- |
|  |  |
| Flow | 0.11 m3/s |
| Width | 570 mm |
| Length | 2000 mm |
| Hand rake | No. 2 |
| Space between bar | 25 mm |
| Bar Type | Rectangular |
| Bar section | 10x30 mm |
| Inclination | 45 Deg |

|  |  |
| --- | --- |
|  |  |
| Frame | AISI 316 |
| Rake | AISI 316 |
| Bar screen | AISI 316 |

|  |  |
| --- | --- |
|  |  |
| Channel Width | 600 mm |
| Depth | 1180 mm |

### 2. Belt Conveyor

|  |  |
| --- | --- |
|  |  |
| Manufacturer | Winkel |
| Quantity | 1 |

|  |  |
| --- | --- |
|  |  |
| Width | 9000 |
| Length | 6000 |

|  |  |
| --- | --- |
|  |  |
| Trade Mark | SEW |
| Model | SA57T |

|  |  |
| --- | --- |
|  |  |
| Trade Mark | SEW |
| Rated Power | 5198.81 |
| Supply Voltage | 380 V, 3 Phases, 50 Hz |
| Insulation | Class F |
| Temp Rise | Class B |
| Ingress Protection | IP65 |

|  |  |
| --- | --- |
|  |  |
| Frame | Hot deep galvanized steel |
| Roller | Hot deep galvanized steel |
| Bolts & Nuts | AISI 304 (A2) |
| Conveyor | Rubber 10 mm (3Ply cotton/nylon) |

### 3. Container

|  |  |
| --- | --- |
|  |  |
| Manufacturer | Factory |
| Quantity | 1 |

|  |  |
| --- | --- |
|  |  |
| Capacity | 2 m3 |
| Thicknesses | 6mm |
| No. of Wheel | 4 |
| Automatic safety lock | Yes |

|  |  |
| --- | --- |
|  |  |
| Frame | Epoxy Coated |
| Bolts & Nuts | Galvanized steel |
| Wheel | Steel with rubber |