Project Name:

testservice

Client Name:

tc

Capacity:

tc

### 1. Manual Screen

|  |  |
| --- | --- |
|  |  |
| Manufacturer | Factory |
| Quantity | 1 |
| Operation | Manual |

|  |  |
| --- | --- |
|  |  |
| Flow | 0.11 m3/s |
| Width | 570 mm |
| Length | 2000 mm |
| Hand rake | No. 2 |
| Space between bar | 25 mm |
| Bar Type | Rectangular |
| Bar section | 10x30 mm |
| Inclination | 45 Deg |

|  |  |
| --- | --- |
|  |  |
| Frame | AISI 316 |
| Rake | AISI 316 |
| Bar screen | AISI 316 |

|  |  |
| --- | --- |
|  |  |
| Channel Width | 600 mm |
| Depth | 1180 mm |